Action: Machine reset

Action: Rejected

Action: Completed

Error: Brush over current

Error: Brush stall

Error: Brush over temp

Error: Side brush over current

Error: Side brush stall

Error: Side brush over temp

Error: Drive motor won’t propel

Error: Drive motor over current

Error: Drive motor stall

Error: Drive motor over temp

Error: Vacuum Over current

Error: Vacuum stall

Error: Vacuum compromised

Error: Circuit board over temp

Error: Unknown

Error: Missing bag

Error: Low battery

Error: Dead battery

Operation mode options

Mode: Transport

Mode: Vacuuming

Mode: Eco vacuuming

Mode: Tool

Alert Options

Alert: Daily

Alert: 50 Hour

Alert: 100 Hour

Alert: 200 Hour

1234567890

1234567890

:30 :15 :45 :00

How-to Guide

How-to Guide  **HOW-TO GUIDE MACHINE STATUS BRUSH DRIVE VACUUM PCB** Machine Status Brush Drive Vacuum PCB

Machine Status Brush Drive Vacuum PCB

Errors Errors

Encapsular R

**MODO**